Solar Photovoltaic (PV) Electrical System Agreement
To be submitted with all requests for PV installations to the Pines I Board of Directors.
I/we have read the Pines I GUIDELINES FOR APPROVAL OF COURTYARD IMPROVEMENTS AND ADDITIONS TO BUILDINGS, regarding PV installations (1-7 listed below) and agree to abide by all 7 requirements.
1. Solar PV electrical systems must sdopt the most current County of Hawaii GUIDELINES FOR PERMITTING A RESIDENTAL PHOTOVOLTAIC (PV) ROOF MOUNTED SYSTEM.   http://www.hawaiicounty.gov/pw-pv-guidelines
2. The owner shall provide the Pines I Board of Directors with a scaled drawingshowing location of major components on the properts necessary to integrate the solar PV array with the site load (building). This includes but is not limited to the solarr panels, array circuit wiring, fusing, emergency disconnect, main panel, meter and power processing equipment.
3. All solar equipment mounted  on common elements (roof, walls, etc.) must have connections to facilitate removal for re-roofing, painting, re-siding and other repairs to the common space elements.
4. All electrical lines shall be routed within the walls or chased in such a manner that avoids exposure. Those portions that are exposed are to be painted to conform to the color of the house or roof.
5. The only solar PV components that can be externally mounted on the common elements (unit roof & external  surfaces) are the solar panels,the emergency responder’s dixconnect switch, main  electrical panel and meter. All other associated equipment, including array circuit wirikng, fusing, disconnects, monitoring devices and power processing equipment may nnot be mounted externally on the common elements. All boxes must be installed inside of the garage.
6. The Emergency Responders Disconnect switch shall belocatedin the immediate vicinity of the HELCO me,ter sercingg the unit. The disconnect switch must be easily accessible to emergency responders and be capable of being locked in the open position.
7. Installation of Sol;ar Photovoltaic PV) electrical Systems must be done by a licensed Solar contractor.

NOTES:   Portions that are exposed are to be painted include any electrical conduits, boxes, roof jacks and dsconnect switches. House color paint codes can be obtained from the managing -agent Property Manager (CAM)..Roof paint is to be exterior flat back.
Owner(s) signature                                                                   Unit #_______        Date __________    
PV Contractor                                                                 License #                               Date __   ______   
 Company name_________________________________ 
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